**Personal Specialisation Project**

Mohammed Nasser Alshukaili.

ICT, Fontys University of Applied Sciences.

Cyber Security, Semester 4.

2022

Contents

[**SCOPE** 3](#_Toc122176559)

[**Main Question** 3](#_Toc122176560)

[**How can Cisco Certified Network Associate (CCNA) certificate prepare me to become a network engineer?** 3](#_Toc122176561)

[Sub Questions 3](#_Toc122176562)

[1- What network fundamentals do I need to take the exam? 3](#_Toc122176563)

[2- How networks can be accessed? 3](#_Toc122176564)

[3- What is IP address and what does it offer? 3](#_Toc122176565)

[4- What security skills do I need to pass the exam? 3](#_Toc122176566)

[5- What is Automation and Programming in the CCNA? 3](#_Toc122176567)

[**My Plan** 3](#_Toc122176568)

[Results 4](#_Toc122176569)

[What network fundamentals do I need to take the exam? 4](#_Toc122176570)

[Network Fundamentals 4](#_Toc122176571)

[Network Access 13](#_Toc122176572)

[References 14](#_Toc122176573)

# **SCOPE**

The aim of this research is to

# **Main Question**

### **How can Cisco Certified Network Associate (CCNA) certificate prepare me to become a network engineer?**

## Sub Questions

### What network fundamentals do I need to take the exam?

### How networks can be accessed?

### What is IP address and what does it offer?

### What security skills do I need to pass the exam?

### What is Automation and Programming in the CCNA?

# **My Plan**

# Results

## What network fundamentals do I need to take the exam?

After browsing Cisco website, I found the content of the CCNA exam. Therefore, I will be relying on that website to study step-by-step for the exam. ([­­­­­­](https://learningnetwork.cisco.com/s/ccna-exam-topics)).

From the website above, here is the content of the current CCNA version:

Graphical user interface, text, application, email

Description automatically generated

### Network Fundamentals

#### Network Topologies

There are many types that people used to design networks. Some of them are:

* Bus Topology
* Ring Topology
* Star Topology

#### Bus Topology

The internet started with 2 devices that were connected using the same cable, this is called Bus Topology. It can handle more than 2 devices as long as they are connected to the same cable.

A picture containing text, sign

Description automatically generated

This design shows that the 3 devices can talk to each other because they use the same cable.

This design is outdated and not used nowadays.

#### Ring Topology

A picture containing text

Description automatically generated

Ring topology is creating a circle with the devices that are connected with each other.

Advantages:

* Network Management: devices can be replaced/removed from the network without shutting it down.
* Cost: Twisted pair cabling is inexpensive and easily available. Therefore, the installation cost is very low.
* Reliable: It is a more reliable network because the communication system is not dependent on the single host computer.

Disadvantages:

* Difficult troubleshooting.
* Delay

#### Star Topology

This design is the most used design these days. The shared device is in the middle, and a cable is going out from it to each device.

Advantages:

* Efficient troubleshooting: troubleshooting is easier than the other designs.
* Easily expandable: more devices can be easily connected to the centered device using its own cable.

Disadvantages:


* A Central point of failure.
* So many cables.

(*Computer Network Topologies - Javatpoint, n.d.)*.

#### OSI MODEL

The Open Systems Interconnection (OSI) is the model that is being used by the modern devices to communicate to other devices on the internet.

The OSI model consists of 7 layers that share the steps of encapsulation/decapsulation.



([*https://www.imperva.com/learn/application-security/osi-model/#:~:text=The%20Open%20Systems%20Interconnection%20(OSI,companies%20in%20the%20early%201980s*)](https://www.imperva.com/learn/application-security/osi-model/#:~:text=The%20Open%20Systems%20Interconnection%20(OSI,companies%20in%20the%20early%201980s)).

Let’s start from the top:

**Layer 7 – Application Layer:**

This layer is where the end-user interacts with a software. Such as, HTTP/S for when visiting a website as in our scenario.

**Layer 6 – Presentation Layer:**

This layer is responsible for encoding, encrypting, and compressing the data that is being sent and received.

**Layer 5 – Presentation Layer:**

It ensures to create communication channels (sessions) to allow the devices to talk to each other. It also ensures that these channels are not being interrupted.

**Layer 4 – Transport Layer:**

This layer turns the data into ordered segments to make sure the data is in the correct order.

It also ensures that the specific segment has been received to send the next one. If a segment was not received, the layer would send it again.

**Layer 3 – Network Layer:**

Network layer breaking up the segments into network packets. Also, it routes the packets to the best path towards the destination.

**Layer 2 – Data Link Layer:**

This layer receives the network packets and turn them into frames, then it sends them to the destination using the Media Access Control to route the frames.

**Layer 1 – Physical Layer:**

It takes care of the physical cables and how the devices are connected and talking to each other.

#### TCP/UDP

TCP requires 2 devices to be connected for them to send packets, therefore TCP is considered connection-based protocol. The following are some of the services that the TCP protocol brings:

* The server ensure that the client received the packets, if not, the server will keep sending the same packet until it is received.
* It uses three-way-handshake to establish a connection.
* Ordered packets
* Reliable

UDP, on the other hand, doesn’t require a connection between the receiver and the sender, therefore, people call it “connectionless”. The UDP has many pros, such as:

* Smaller packets
* Less bandwidth
* Fast

(BasuMallick, 2022).

##### TCP

Let’s talk about how TCP works.

Scenario 1:

Let’s assume that I am on my PC, and I want to access git.fhict.nl.

I open google and I type:

Graphical user interface, text, application

Description automatically generated

It will send me to the git page that I asked for. However, I want to discuss what happens behind the scenes that led to showing the page.

After pressing Enter, a PDU information that consists of 7 layers will be sent to the destination server. What is inside the 7 layers?

**Layer 7:**

Layer 7 will tell the server that I sent HTTPs request, this helps the server to route me to the web page.

The PDU will look like this after this layer:

Graphical user interface, application

Description automatically generated

This means that application layer completed its data, and the other layers are waiting.

**Layer 4:**

Transport layer is where the port information is stored. As we are requesting a web page, layer 4 will carry TCP as header + the port that we are connecting to:

Graphical user interface, text

Description automatically generated

Now this is called a segment.

**Layer 3:**

The network layer carries the information about the source IP address and the destination IP address.

Text

Description automatically generated

Now this packet has all the previous information PLUS the IP addresses.

**Layer 2:**

Layer 2 will take all the information before and add the MAC addresses. After adding the Layer 2 header and trailer, it will be called “Frame”.

Text

Description automatically generated

Now all these information are stored in one “envelope” this letter is ready to be sent using the Ethernet cable which we cover in the next layer.

Layer 1:

Physical layer is the connection cable that will take all the previous information and send them to the internet.

After the message is received by the destination, then it will **decapsulate** the letter to reveal the layers information.

The web server will **decapsulate** the layers just to find out that they carry information for the server itself. The server will find its MAC address in layer 2, its IP address in layer 3, port TCP in layer 4, and HTTPs in layer 7, then it will send back the web page. (NetworkChuck, 2020a)

#### Subnetting

Subnetting is the strategy used to create separate networks inside one network.

When you have one network and 100 employees, you would not want all the employees to be in the same network. Therefore, network engineers divide that one network into many sub-networks.

Then, a sub network can be given to several employees that share the same job like marketing, business, and information technology.

**Subnet masks:**

*CLASS A:* 255.0.0.0 (Number of hosts possible: 255\*255\*255 = 16581375)

*CLASS B:* 255.255.0.0. (Number of hosts possible: 255\*255 = 65025)

*CLASS C:* 255.255.255.0 (Number of hosts possible = 255)

Why subnetting is important?

* It helps to reduce the traffic by splitting the network into many.
* It helps to divide the hosts as wanted.
* It helps employees to work from home without needing to connect to the open network.

(Techopedia, 2017).

Let’s understand subnetting by answering some questions:

**What is the broadcast address for 223.209.177.136/29?**

The broadcast is the last IP address for a specific network. The question gives us a single IP in that network. How do we know how many hosts are in that network to find the last IP?

Subnet mask can help us here.

Subnet mask = 29 = (29 1s then the rest are zeros) = 11111111.11111111.11111111.11111000

= 255.255.255.248

Text

Description automatically generated

What is the network ID for 221.230.76.99/27 ?

Network ID is the first IP in a network.

First, we need to figure out the number of hosts possible in this network.

/27 = 11111111.11111111.11111111.11100000

Hosts = 2 to the power of 5 = 32.

Text

Description automatically generated

**You have 209.51.44.0/24, you need to subnet into 5 networks. What is your new subnet mask?**

/24 = 11111111.11111111.11111111.00000000

This equals 2 to the power of zero = 1 network possible.

I need 5 networks. Therefore, I need to borrow from the host portion. If I borrow only one zero, it will give me 2 to the power of 1 = 2 networks.

If I borrow 2 zeros, it will give me 2 to the power of 2 networks = 4 networks, still not enough.

If I borrow 3, it will give me 2 to the power of 3 = 8 networks possible.

Text

Description automatically generated

(ITProTV, 2022)

#### Cisco Packet Tracer

I will take advantage of the Cisco Packet Tracer to understand how online devices communicate behind the scenes.

Cisco Packet Tracer can be downloaded from here:

<https://www.netacad.com/courses/packet-tracer>

Once you open the application, you will find a dashboard that helps you with simulating a network.

Graphical user interface, application

Description automatically generated

Let me start with creating a simple network that consists of 2 PCs and one switch.

Chart

Description automatically generated

Now the 2 PCs are connected to the same switch. However, they can not talk to each other yet due to the fact they do not have IP addresses yet.

Let me configure each PC to have its own IP address.

**PC0**

Graphical user interface, text, application, email

Description automatically generated

**PC1**

Graphical user interface, text, application, email

Description automatically generated

Now that the 2 end points have IP addresses, let me try to ping one device to another:

Graphical user interface, application

Description automatically generated

On the PC0 device, I am trying to ping PC1. So far there is no response because I need to resume the simulation.

After forwarding the message,

Diagram

Description automatically generated with low confidence

There is an envelope going from PC0 to the switch that carries the information for the ping.

Let me see what is inside that message:

Graphical user interface, text, application

Description automatically generated

The switch operates on layer 2, this is why it can only see the MAC address of the source and destination.

After forwarding the message from the switch to the final destination, PC1 can open all the layers messages as it is the final destination.

Graphical user interface, text, application, email

Description automatically generated

### Network Access

#### VLAN

What is VLAN?

A virtual LAN is a logical concept that connects devices that share the same purpose together. Then, the devices that are in the same VLAN are in a different sub-network that other devices. Grouping them helps to isolate the traffic for each sub-network.

Why is VLAN important?

Network engineers tend to use VLANS for some of the following reasons:

* To strengthen the security
* To reduce the unnecessary traffic
* To improve performance
* Easier to administrate

**Security**

VLANS can help with improving the security by controlling which devices have access to other devices. Administrators can strict the connections between these devices, and only allow the devices that need each other to send data between them

**Reduce unnecessary traffic**

Dividing the devices into VLANS means that marketing devices does not know anything about the traffic that business devices are sending and receiving. This improves the flow of the traffic in the network as each sub-network can only have access to what it needs.

**Improve performance**

Less traffic leads to better performance. VLANS reduce the number of other devices that keep sending broadcast.

Engineers can also prioritize traffic against another. For instance, VLANS that consists of voice over IP can prioritize this traffic to improve the performance, and isolate other devices on a different VLAN.

**Administration**

Grouping devices that share the same purpose can help with administrating them. Network engineers can them navigate to one VLAN and start administrating.

(Slattery & Burke, 2022)

How to create VLANS?

End-point devices that are connected to the same switch can be divided into multiple VLANS. For instance, in a small company, marketing, business, security devices are connected to the same switch, this causes unnecessary traffic for the different sections. Creating VLANS can be by specifying the ports to a unique VLAN.

Diagram

Description automatically generated

This picture illustrates that one switch can create more than one VLAN. Each color represents a VLAN that consists of the devices that are connected to that color.

What happens if we want to add a device that is connected to another switch to a VLAN in this switch?

**Trunk**

Trunk is connecting a switch to another switch via a physical cable. This will allow all the devices that are connected to one switch communicate with devices that are connected with the other switch.

Diagram

Description automatically generated

Now a single VLAN can be created for each color.

Let me apply this in a practice lab.

Diagram

Description automatically generated

Cisco IP Phone is connected to NYCORE2 switch. I want to create 2 VLANS in that switch, one for voice, and one for data.

Text

Description automatically generated

Here are the commands that I would need to create VLANS in a switch. Now that I created 2 VLANS (Voice and Data) and they are both active, notice that I did not assign any ports for these VLANS.

With the following commands, I can assign specific ports to the 2 VLANS that I created earlier.

Text

Description automatically generated

As you can see, Voice and Data VLANS are now connected to the same port.

# References

* BasuMallick, C. (2022, April 18). *TCP vs. UDP: Understanding 10 Key Differences*. <https://www.spiceworks.com/tech/networking/articles/tcp-vs-udp/>
* *Computer Network Topologies - javatpoint*. (n.d.). www.javatpoint.com. <https://www.javatpoint.com/computer-network-topologies>
* NetworkChuck. (2020a, August 6). *REAL LIFE example!! (TCP/IP and OSI layers) // FREE CCNA // EP 4*. YouTube. https://www.youtube.com/watch?v=3kfO61Mensg
* Techopedia. (2017, July 18). Subnetting. Techopedia.com. <https://www.techopedia.com/definition/28328/subnetting>
* ITProTV. (2022). <https://app.itpro.tv/login/?redirect_to=%2Fcourse%2Fcisco-ccna-200-301-2022%2Fperforming-class-c-ipv4-subnetting>
* Slattery, T., & Burke, J. (2022, June 3). *VLAN (virtual LAN)*. Networking. <https://www.techtarget.com/searchnetworking/definition/virtual-LAN>
* *Cisco Packet Tracer*. (2022, June 17). Networking Academy. <https://www.netacad.com/courses/packet-tracer>